Set of characteristics for each product offered for your boiler or sale - one form per ‘product definition’. All the products in the Woodsure scheme must have a completed form.

Please ensure the correct supporting RBRA document for RHI is in place.

Firewood and Woodchip

|  |  |
| --- | --- |
| Business Name:  | WS number:  |
| Product Definition- Choose one from each column  Drying Type: ¨ Force Dried Fuel Type: ¨ Hardwood  ¨ Seasoned ¨ Softwood ¨ Mixed |
| Please specify the maximum log length indicated on your boiler manual or your customers Length of log:  | Choose the woodchip/hog size according to BS EN ISO 17225 standardsWoodchip/ Hog: ¨ P16S ¨ P31S ¨ P45S ¨ P63S |
| Moisture Content: ¨M20 ¨M25 ¨M30 ¨M35 ¨M40  |
| Class of fuel : ¨A1 ¨A2 ¨B1 ¨B2 |

\*A1 – virgin wood and chemically untreated wood residues with low ash content (little or no bark).

A2 - virgin wood and chemically untreated wood residues with a higher ash content

B1 – includes other material such as short rotation coppice, wood from gardens and plantation and chemically untreated industrial by-products and residues.

B2 - includes chemically treated industrial by products and residues and used wood. Timber that has heavy metals or halogenated organic compounds are excluded

Briquette

|  |  |
| --- | --- |
| Business Name:  | WS Number: |
| Brand Name/Briquette Type: |
| Please specify the maximum briquette length and diameter indicated on your boiler manual or your customers Length of Briquette:Diameter:  | From the following options, please choose the wood fuel product used in the briquette¨ Hardwood ¨ Softwood¨ Mixed  |
| Moisture content: ¨M5 ¨M10 ¨M15 ¨M20  |
| Class of fuel : ¨A1 ¨A2 ¨B ¨Ungraded |

\*A1 – virgin wood and chemically untreated wood residues with low ash content (little or no bark).

A2 - virgin wood and chemically untreated wood residues with a higher ash content

B1 – includes other material such as short rotation coppice, wood from gardens and plantation and chemically untreated industrial by-products and residues.

B2 - includes chemically treated industrial by products and residues and used wood. Timber that has heavy metals or halogenated organic compounds are excluded